BSPD V2

Focus on noise elimination, differential with return ground line?

Requires negative voltage rail?

Two boards?

Main board and sensor interface board, interface board to read current sensor and provide stable offset reference to send back to main board differential.

Reverse polarity of comparator inputs in case of chip failure