Concentric Twist Notes

# Diameters

|  |  |
| --- | --- |
| 20 gauge | 1.5 |
| Twisted 20 gauge | 2.5 |
| Dual Twisted 20 gauge core  (2 twisted pairs twisted together | 3.7 |

Lay Direction: Left hand lay passes from right to left as it passes over the top of the cable

Conventional for final layer to be LH lay