Autosport Stock

## Requirements

From Enclosure Connections Document

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Connector** | **Quantity and Configuration** | | | |
|  | **A** | **B** | **C** | **D** |
| Size 10 - 6 x size 20 contacts | 10 | 6 |  |  |
| Size 12 - 10 x size 20 contacts | 6 | 2 |  |  |
| Size 14 - 19 x size 20 contacts | 1 | 2 | 2 |  |
| Size 22 – ASHD 2x#4 3x#20 |  |  |  | 4 |

## Current Stock

Refer to Race Spec Order PDF for full list.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Connector** | **Quantity and Configuration** | | | |
|  | **A** | **B** | **C** | **D** |
| Size 10 - 6 x size 20 contacts | 9 | 6 |  |  |
| Size 12 - 10 x size 20 contacts | 7 | 3 |  |  |
| Size 14 - 19 x size 20 contacts | 5 | 3 | 2 |  |
| Size 22 – ASHD 2x#4 3x#20 |  |  |  | 3 |

## Difference

To be purchased, requirements - stock

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Connector** | **Quantity and Configuration** | | | |
|  | **A** | **B** | **C** | **D** |
| Size 10 - 6 x size 20 contacts | 1 | 0 |  |  |
| Size 12 - 10 x size 20 contacts | -1 | -1 |  |  |
| Size 14 - 19 x size 20 contacts | -4 | -1 | 0 |  |
| Size 22 – ASHD 2x#4 3x#20 |  |  |  | 1 |

## Connector Configurations

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Configuration** | **A** | **B** | **C** | **D** |
| Keyway | N | A | N | N |
| Socket-Pin Arrangement | Pin-receptacle 0P  Socket-plug 6S | Pin-receptacle 0P  Socket-plug 6S | Socket-receptacle 0S  Pin-plug 6P | Pin-receptacle 0P  Socket-plug 6S |

0 = Receptacle, 6 = Free Plug

P = Pin, S = Socket