CAN Node Minor

# Requirements

* 2x CAN bus enables
* 8x standard analog inputs
* 8x digital inputs
* 2x thermocouple capability
* Level shifting/Zener drops
* 5V buck converter supply
* 8x power
* 8x gnd